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Maxidirect Verification Method

For checking the wave lengths with your verification standards, please select the following method no:
[image: cid:0123-0029-0E-0B-TJ-6]
 
The required wavelength is on a sticker on the coloured vials. 
1. Place the zero vial in the chamber and press ZERO. 
2. Place a standard vial in the chamber e.g. 430 nm for method 900 and press TEST. 
[bookmark: _GoBack]3. Compare the result with the value on the enclosed verification certificate. 
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Method-No. Title
900 mAbs 430 nm
910 mAbs 530 nm
920 mAbs 560 nm
930 mAbs 580 nm
940 mAbs 610 nm
950 mAbs 660 nm
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